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[bookmark: __RefHeading___Toc381357623]REQUEST FOR QUOTATION

  
Date: 12th October, 2026


Contract Name: Construction of 1NO. CHPS Compound at Alhassan Akura in the Kintampo Municipality


Contract Number: BER/KiMA/WKS/PQ/20/26

1. The Kintampo Municipal Assembly intends to apply part of its budgetary allocation to fund the procurement of the following works: Construction of 1No. CHPS Compound at Alhassan Akura.

2. The Kintampo Municipal Assembly hereby invites sealed Quotations from Contractors for the Construction of 1No. CHPS Compound at Alhassan Akura. The duration for the works is Eight (8) Months.

3. It is mandatory that Tenderers include in their tender the underlisted statutory requirements.

· Valid Business Registration Certificate 
· Certificate of Incorporation and Commencement (For Companies)
· Valid GRA Tax Clearance Certificate
· Valid SSNIT Clearance Certificate. 
· Valid Works and Housing Certificate (D3K3)
· Valid Labour Certificate
· Power of Attorney where applicable
· Valid Registration Certificate from PPA

4. Eligible Tenderers interested in obtaining the Request for Quotation documents may obtain further information and inspect the Tender Documents on Ghana Electronic Procurement System (GHANEPS) from Monday, 12th October, 2026. 

5. A complete set of Request for Quotation Documents in English may be obtained and submitted electronically by interested tenderers through: https://www.ghaneps.gov.gh/epps/app/searchplan.do.

6. The deadline for submission of Tenders is Monday, 19th October, 2026 at 10:00am.      Tenders must be delivered electronically on or before the time specified above. 
 	
	

	





____________________
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[bookmark: __RefHeading___Toc381357626][bookmark: _Toc240918306]Section I.  Instructions to Prospective Contractors
[bookmark: __RefHeading___Toc381357627][bookmark: _Toc240918307]A.  General
	[bookmark: __RefHeading___Toc381357628][bookmark: _Toc240918308]Definitions
	  “QDS” means Quotation Data Sheet in Section II of these Request for Quotation Documents used to reflect specific requirements and/or conditions.
“Request for Quotation” means a Request for Quotation for the provision of the Works submitted by a Request for Prospective Contractor in response to these Request for Quotation Documents.
 Prospective Contractor” means any eligible entity or person, including any associate of such eligible entity or person that submits a Request for Quotation.
Request for Quotation Documents” means Sections these documents, including any amendments that may be made, prepared by the Employer for the selection of the Contractor.
“Bill of Quantities” means the priced and completed Bill of Quantities forming part of the Request for Quotation.
 “Confirmation” means confirmation in writing.
“Contract” means the contract proposed to be entered into between the Employer and the Contractor, including all of the documents specified in GCC Sub-Clause 2.3 and any attachments, appendices, and all documents incorporated by reference therein.
“Contract Price” means the price stated in the Letter of Acceptance and thereafter as adjusted in accordance with the provisions of the Contract.
“Contractor” means the entity or person, including any associate, that provides the Works to the Employer under the Contract.
“Day” means a calendar day.
“Employer” means the entity inviting the Quotations, the party with which the Contractor signs the Contract for the provision of the Works.
Defines, for the purposes of this provision, the terms set forth below as follows:
i. “Corrupt practice” is the offering, giving, receiving, or soliciting, directly or indirectly, of anything of value to influence improperly the actions of another party;
ii. “Fraudulent practice” is any act or omission, including misrepresentation, that knowingly or recklessly misleads, or attempts to mislead, a party to obtain financial or other benefit or to avoid an obligation;
iii. “Collusive practice” is an arrangement between two or more parties designed to achieve an improper purpose, including to influence improperly the actions of another party;
iv. “Coercive practice” is impairing or harming, or threatening to impair or harm, directly or indirectly, any party or the property of the party to influence improperly the actions of a party;
v. “Obstructive practice” is:
deliberately destroying, falsifying, altering, or concealing of evidence material to the investigation or making false statements to investigators in order to materially impede an investigation into allegations of a corrupt, fraudulent, coercive, or collusive practice; and/or threatening, harassing, or intimidating any party to prevent it from disclosing its knowledge of matters relevant to the investigation or from pursuing the investigation; or
acts intended to materially impede the exercise of the PPA’s inspection and audit rights.
Rejects a proposal for award if the Entity determines that the firm or individual recommended for award, any of its personnel, or its agents, or its sub-consultants, sub-contractors, service providers, suppliers and/ or their employees, has, directly or indirectly, engaged in corrupt, fraudulent, collusive, coercive, or obstructive practices in competing for the contract in question;

 “GCC” means the General Conditions of Contract.
“Government” means the Government of Ghana.
“Instructions to Prospective Contractors or “ITPC” mean this Section I of these Request for Quotation Documents, including any amendments, which provide Prospective Contractors with information needed to prepare their Quotations.
“Intended Completion Date” means the date on which it is intended that the Contractor shall complete the Works as specified in RQDS.
“in writing” means communicated in written form (e.g., by mail, e-mail or facsimile) delivered with proof of receipt.
“Letter of Acceptance” has the meaning given the term in RQDS.
“PPA” means the Public Procurement Authority
 “SCC” means the Special Conditions of Contract.
 “Taxes” has the meaning given the term in Table C.
 “Works” means what the Contract requires the Contractor to construct, install, and turn over to the Employer.

	[bookmark: __RefHeading___Toc381357629][bookmark: _Toc240918309]Scope of Request for Quotation
	1.1 The Works for which the Request for Quotation Documents have been issued is:    Construction of 1No. CHPS Compound at Alhassan Akura in the Kintampo Municipality  
1.2 The identification number of this Request for Quotation process is:  BER/KiMA/WKS/PQ/20/26 
1.3 The number and identification of lot (contract) comprising this IFT is: [insert number and identification of each lot, if applicable]  

1.4 Throughout these Request for Quotation Documents, except where the context requires otherwise, words indicating the singular also include the plural and words indicating the plural also include the singular; and the feminine means the masculine and vice versa.

	[bookmark: __RefHeading___Toc381357630][bookmark: _Toc240918310]Source of Funds 
	The Employer intends to apply a portion of its budgetary allocation to fund payments under the Contract for which these Request for Quotation Documents are issued.

	[bookmark: __RefHeading___Toc381357631][bookmark: _Toc240918311]Fraud and Corruption
	The Employer requires that all beneficiaries of its funding, including any   Contractors, suppliers, contractors, subcontractors and consultants observe the highest standards of ethics during the procurement and execution of this contract.   
In line with this, the Employer:
will reject a Quotation if it determines that the Request for Prospective Contractor recommended to be selected as the Contractor has, directly or indirectly, engaged in Fraud and Corruption in competing for the Contract;
has the right to sanction a Request for Prospective Contractor, including declaring the Prospective Contractor ineligible, either indefinitely or for a stated period of time, to be awarded a contract if at any time it determines that the Prospective Contractor or Contractor has, directly or through an agent, engaged in Fraud and Corruption in competing for, or in executing, such a contract; and
Furthermore, Prospective Contractors shall be aware of the provisions stated in Section V, General Conditions of Contract (GCC).

	[bookmark: __RefHeading___Toc381357652][bookmark: _Toc240918312]Cost of Request for Quotation
	The Prospective Contractor shall bear all costs associated with the preparation and submission of its Request for Quotation, and the Employer shall, in no case, be responsible or liable for those costs, regardless of the conduct or outcome of the Request for Quotation process.  


[bookmark: __RefHeading___Toc381357653][bookmark: _Toc240918313]B.  Request for Quotation Documents
	[bookmark: __RefHeading___Toc381357655][bookmark: _Toc240918314]Contents of Request for Quotation  Documents
	The set of Request for Quotation Documents comprises the documents listed below and addenda issued in accordance with ITT Clause 10:
Part I —Request for Quotation Request for Quotation Procedures
Section I. Instructions to Request for Contractor Prospective Contractors (ITRQ)
Section II. Request for Quotation
Section III. Evaluation and Qualification Criteria
Section IV.  Request for Quotation Forms
Part II – Forms of Contract 
Section V.  General Conditions of Contract (GCC)
Section VI. Form of Special Conditions of Contract (SCC)
Section VII.  Forms of Agreement 
Part III -- Works Requirements
Section VIII.  Bill of Quantities (Appendix 1)
Section IX. Specifications and Performance Requirements (Appendix 2)
Section X.  Drawings (Appendix 3)
The Prospective Contractor is expected to examine all instructions, forms, terms, and specifications, inclusive of environmental, social and health and safety requirements, in the Request for r Quotation Documents.  Failure to furnish all information or documentation required by the Request for Quotation Documents may result in the rejection of the Request for Quotation.

	[bookmark: __RefHeading___Toc381357656][bookmark: _Toc240918315]Clarification of Request for Quotation Documents
	A prospective Contactor requiring any clarification of the Request for Quotation Documents may notify the Employer in writing at the Employer’s address indicated in these Documents.  The Employer will respond, in writing, to any request for clarification received earlier than the number of days indicated in these prior to the deadline for submission of Quotations.  Copies of the Employer’s response will be forwarded to all prospective Contractors who have acquired the Request for Quotation Documents.  

	
	


[bookmark: __RefHeading___Toc381357658][bookmark: _Toc240918316]C.  Preparation of Quotations
	
	

	[bookmark: __RefHeading___Toc381357661][bookmark: _Toc240918317]Documents Comprising the Request for Quotation
	The Quotation submitted by Prospective Contractor shall comprise the following:
The Request for Quotation (in the format indicated in Section IV);
Request for Quotation Priced Bill of Quantities;
Technical Offer/Method Statement;
Written power of attorney authorizing the signatory of the response to the Request for Quotation to commit the Prospective Contractor, in accordance with ITT 11.2; and
Any other materials required to be completed and submitted by Request for Prospective Contractors. 

	[bookmark: __RefHeading___Toc381357662][bookmark: _Toc240918318]Request for Quotation Prices
	The Contract shall be for the Works, as described in ITT Sub-Clause 1.1, based on the priced Bill of Quantities or priced Schedule of Activities submitted by the Request for Quotation for Prospective Contractor.
The Prospective Contractor shall fill in rates and prices for all items of the Works described in the Bill of Quantities.  Items for which no rate or price is entered by the Request for Prospective Contractor shall not be paid for by the Employer when executed and shall be deemed covered by the other rates and prices in the Bill of Quantities.  Corrections, if any, shall be made by crossing out, initialing, dating and rewriting.
Table C sets forth the tax provisions applicable to any Request for Quotation and to performance of the Contract.  Request for Quotation for Prospective Contractors should review and consider this clause carefully in preparing their Request for Quotation.  
The rates and prices quoted by the Prospective Contractor shall be subject to adjustment during the performance of the Contract if provided for in the RQDS and SCC and the provisions of Clause 11.8 of the GCC.  The Prospective Contractor shall submit with the Request for Quotation all the information required under the SCC and GCC Clause 11.8.

	[bookmark: __RefHeading___Toc381357663][bookmark: _Toc240918319]Request for Quotation
	Request for Quotation

	[bookmark: __RefHeading___Toc381357664][bookmark: _Toc240918320]Request for Quotation Validity
	Request for Quotations shall remain valid for the period specified in the RQDS. A Request for Quotation valid for a shorter period shall be rejected by the Employer as non-responsive.
In exceptional circumstances, prior to the expiration of the original Request for Quotation validity period, the Employer may request Prospective Contractors to extend the period of validity of their Request for Quotations for a specified additional period.  The request and the Request for the Prospective Contractors’ responses shall be made in writing.  A Prospective Contractor agreeing to the request shall not be required or permitted to modify its Request for Quotation, except at the discretion of the Employer.
In the case of fixed price contracts, if the award is delayed by a period exceeding sixty (60) days beyond the expiry of the initial Request for Quotation validity period, the contract price will be increased by a factor specified in the request for extension. The Request for Quotation evaluation shall be based on the Request for Quotation price without taking into consideration the above correction.

	
	

	[bookmark: __RefHeading___Toc381357672][bookmark: _Toc240918321]Format and Signing of Request for Quotation
	The Prospective Contractor shall prepare one original set of the documents comprising the Request for Quotation as described in ITT 13 and clearly mark it ORIGINAL. In addition, the Prospective Contractor shall submit copies of the Request for Quotation in the numbers specified in the TDS and clearly mark each one COPY.  In the event of any discrepancy between the original and the copies, the original shall prevail. 
The original and all copies of the Request for Quotation shall be typed or written in indelible ink and shall be signed by a person duly authorized to sign on behalf of the Prospective Contractor.  This authorization shall consist of a written confirmation as specified in the RQDS and shall be attached to the Request for Quotation. The name and position held by each person signing the authorization must be typed or printed below the signature.  All pages of the Request for Quotation where entries or amendments have been made shall be signed or initialed by the person signing the Request for Quotation.
Any inter-lineation, erasures, or overwriting shall be valid only if they are signed or initialed by the person signing the Request for Quotation.
The Prospective Contractor shall furnish information as described in Section IV – Request for Quotation Forms on commissions or gratuities, if any, paid or to be paid to agents relating to this Request for Quotation, or to Contract execution if the Request for Quotation for Prospective Contractor is awarded the Contract.
Request for Quotations shall be submitted strictly in accordance with the Request for Quotation Documents.  Any amendments or qualifications made by the Prospective Contractor, except those to comply with instructions issued by the Employer, may result in rejection of the Request for Quotation.


[bookmark: __RefHeading___Toc381357673][bookmark: _Toc240918322]D.  Submission of Request for Quotations
	[bookmark: __RefHeading___Toc381357675][bookmark: _Toc240918323]Submission, Sealing, and Marking of Request for Quotations
	Prospective Contractors may always submit their Quotations by mail or by hand.  Prospective Contractors submitting Request for Quotations electronically shall follow the procedures specified in the RQDS. For Request for Quotations submitted in hard copy, the Prospective Contractor shall seal the original and all copies of the Quotation in two inner envelopes and one outer envelope, duly marking the inner envelopes as “ORIGINAL” and “COPIES.”
The inner and outer envelopes shall:
(a) bear the name and address of the Prospective Contractor;
(b) be addressed to the Employer at the address provided in the RQDS;
(c) bear the name and identification number of the Contract as defined in the RQDS and SCC; and
(d) provide a warning” DO NOT OPEN BEFORE” the specified time and date for Request for Quotation opening as defined in the TDS.
If the envelopes are not sealed and marked as above, the Employer shall assume no responsibility for the misplacement or premature opening of the Request for Quotation.

	[bookmark: __RefHeading___Toc381357676][bookmark: _Toc240918324]Deadline for Submission of Request for Quotations
	Request for Quotations shall be delivered to the Employer at the address specified above no later than the time and date specified in the RQDS.
The Employer may, at its discretion, extend the deadline for submission of Request for Quotations by issuing an addendum in accordance with ITT Clause 10, in which case all rights and obligations of the Employer and the Prospective Contractors previously subject to the original deadline shall then be subject to the new deadline.

	[bookmark: __RefHeading___Toc381357677][bookmark: _Toc240918325]Late Request for Quotations
	Any Request for Quotation received by the Employer after the deadline prescribed in ITT Clause 19 shall be declared late, rejected, and returned unopened to the Request for Quotation for Prospective Contractor.

	
	


[bookmark: __RefHeading___Toc381357679][bookmark: _Toc240918326]E.  Request for Quotation Opening and Evaluation
	[bookmark: __RefHeading___Toc381357681][bookmark: _Toc240918327]Request for Quotation Opening
	The Employer shall open the Quotations, including modifications made pursuant to ITT Clause 21, in the presence of the Prospective Contractors’ representatives who choose to attend at the time and in the place specified in the RQDS.  
The Employer shall prepare minutes of the Quotation opening, including the information disclosed, to those present. 

	[bookmark: __RefHeading___Toc381357682][bookmark: _Toc240918328]Confidentiality
	Information relating to the examination, clarification, evaluation, and comparison of Quotations and recommendations for the award of a Contract shall not be disclosed to Prospective Contractors or any other persons not officially concerned with such process until publication of the award to the successful Contractor has been announced.  The undue use by any Prospective Contractor of confidential information related to the process may result in the rejection of its Quotation and may subject the Prospective Contractor to the provisions of the Government’s and the Employer’s anti-fraud and corruption policies.
Any effort by a Prospective Contractor to influence the Employer’s processing of Request for Quotations or award decisions may result in the rejection of its Request for Quotation. Notwithstanding the above, from the time of Request for Quotation opening to the time of Contract award, if any Prospective Contractor wishes to contact the Employer on any matter related to the Request for Quotation process, it should do so in writing.

	[bookmark: __RefHeading___Toc381357683][bookmark: _Toc240918329]Clarification of Request for Quotations 
	To assist in the examination, evaluation, and comparison of Request for Quotations, the Employer may, at its discretion, ask any Prospective Contractor for clarification of the Prospective Contractor’s Request for Quotation, including breakdown of prices. The request for clarification and the response shall be in writing, but no change in the price or substance of the Request for Quotation shall be sought, offered, or permitted except as required to confirm the correction of arithmetic errors discovered by the Employer in the evaluation of the Request for Quotations in accordance with ITT Clause 26.

	
	

	[bookmark: __RefHeading___Toc381357685][bookmark: _Toc240918330]Correction of Errors
	Request for Quotations determined to be substantially responsive shall be checked by the Employer for any arithmetical errors and corrected on the following basis:
(a) if there is a discrepancy between the unit price and the total price that is obtained by multiplying the unit price and quantity, the unit price shall prevail and the total price shall be corrected, unless in the opinion of the Employer there is an obvious misplacement of the decimal point in the unit price, in which case the total price as quoted shall govern and the unit price shall be corrected; 
(b) if there is an error in a total corresponding to the addition or subtraction of subtotals, the subtotals shall prevail and the total shall be corrected; and
(c) if there is a discrepancy between words and figures, the amount in words shall prevail, unless the amount expressed in words is related to an arithmetic error, in which case the amount in figures shall prevail subject to (a) and (b) above.

[bookmark: _Ref201635974]If the Prospective Contractor that submitted the lowest-evaluated Request for Quotation does not accept the correction of errors, its Request for Quotation shall be rejected. 

	[bookmark: __RefHeading___Toc381357686][bookmark: _Toc240918331]Request for Quotation
	Request for Quotation

	[bookmark: __RefHeading___Toc381357687][bookmark: _Toc240918332]Evaluation and Comparison of Request for Quotations
	The Employer shall evaluate and compare only the Request for Quotations determined to be substantially responsive in accordance with ITT Clause 25.  
In evaluating the Request for Quotations, the Employer shall determine for each Request for Quotation the evaluated Request for Quotation price by adjusting the Request for Quotation price as follows:
Making any correction for errors pursuant to ITT Clause 26;
Excluding provisional sums and the provision, if any, for contingencies in the Bill of Quantities, but including day works, where priced competitively;
Making an appropriate adjustment for any other acceptable variations, or deviations submitted.
Making appropriate adjustments to reflect discounts or other price modifications offered in accordance with ITT Sub-Clause 21.5; and
The evaluation factors indicated in Section III - Evaluation and Qualification Criteria.
The Employer shall determine to its satisfaction whether the Prospective Contractor that is selected as having submitted the lowest evaluated and substantially responsive Request for Quotation is qualified to perform the Contract satisfactorily.  The determination shall be based upon an examination of the documentary evidence of a Prospective Contractor’s qualifications submitted by a Prospective Contractor and the qualification criteria indicated in Section III - Evaluation and Qualification Criteria.
The Employer reserves the right to accept or reject any variation, deviation, or unsolicited alternative offer.  Variations, deviations, and unsolicited alternative offers and other factors which are in excess of the requirements of the Request for Quotation Documents or otherwise result in unsolicited benefits for the Employer shall not be taken into account in Request for Quotation evaluation.  
The estimated effect of any price adjustment conditions under GCC Clause 11.8, during the period of implementation of the Contract, shall not be taken into account in Request for Quotation evaluation.
At any time during the evaluation process, the Employer reserves the right to conduct a verification of market-reasonableness of the prices offered, and a negative determination (either unreasonably high or unreasonably low) could be a reason for rejection of the Request for Quotation at the discretion of the Employer.  The Prospective Contractor shall not be permitted to revise its Request for Quotation after this determination.

	
	

	[bookmark: __RefHeading___Toc381357689][bookmark: _Toc240918333]Determination of the Lowest Evaluated Request for Quotation
	The Request for Quotation with the lowest evaluated price from among those which are eligible, compliant and substantially responsive shall be the lowest evaluated Request for Quotation.


[bookmark: __RefHeading___Toc381357690][bookmark: _Toc240918334]F.  Award of Contract
	[bookmark: __RefHeading___Toc381357691][bookmark: _Toc240918335]Award Criteria

	Prior to the expiration of the period of Request for Quotation validity, the Employer will award the Contract to the Prospective Contractor whose Request for Quotation has been determined to be substantially responsive to the Request for Quotation Documents and who has offered the lowest evaluated Quotation price, provided that such Request for Prospective Contractor has been determined to be (a) eligible. (b) qualified and (c) otherwise determined qualified to perform the Contract.

	
	

	[bookmark: __RefHeading___Toc381357693][bookmark: _Toc240918336]Employer’s Right to Accept any Request for Quotation and to Reject any or all Request for Quotations
	The Employer reserves the right to accept or reject any Quotation, at any time prior to the award of Contract, without thereby incurring any liability to any Prospective Contractor or any obligation to inform the affected Prospective Contractors of the grounds for the Employer’s action.

	[bookmark: __RefHeading___Toc381357694][bookmark: _Toc240918337]Employer’s Right to cancel the Request for Quotation process and reject all Request for Quotations
	The Employer reserves the right to cancel the Request for Quotation process and reject all Request for Quotations, at any time prior to the award of Contract, without thereby incurring any liability to any Prospective Contractor or any obligation to inform the affected Prospective Contractor or of the grounds for the Employer’s action.

	
	

	[bookmark: __RefHeading___Toc381357696][bookmark: _Toc240918338]Notification of Award and Signing of Agreement
	The Prospective Contractor whose Quotation has been accepted shall be notified of the award by the Employer in writing prior to the expiration of the Request for Quotation validity period using a letter of acceptance substantially in the form set out in Section VII of these Request for Quotation Documents (the “Letter of Acceptance”). 
The Letter of Acceptance shall constitute the formation of the Contract, subject to the Prospective Contractor signing the Contract. 
The Contract will constitute all agreements between the Employer and the successful Contractor as described in SCC Clause 1.1.1.   Promptly after providing the successful Contractor with the Letter of Acceptance, the Employer will send the successful Contractor the Agreement.  Within 7 days of receipt, the successful Contractor shall sign the Contract and deliver it to the Employer.
Upon the successful Contractor furnishing of the performance security the Employer will promptly notify unsuccessful Contractors the name of the winning Contractor and the Contract amount.

	
	After publication of the award, unsuccessful Contractors may request in writing to the Employer for a debriefing seeking explanations for the failure of their Request for Quotations.  The Employer shall promptly respond in writing to any unsuccessful Contractor who, after notification of award, requests of the Employer in writing the grounds on which its Quotation was not selected.
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SECTION II.  REQUEST FOR QUOTATION DATA SHEET
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	[bookmark: _Toc240918340]A.  General
	

	


Definitions
	 “Employer” means:  Kintampo Municipal Assembly  
“Government” means the Government of Ghana. 
	

	

ITT 1.1
	The Works for which the Request for Quotation Documents have been issued is:    Construction of 1No. CHPS Compound at Alhassan Akura in the Kintampo Municipality  
The identification number of this Request for Quotation process is:  BER/KiMA/WKS/PQ/20/26
The number and identification of lot (contract) comprising this IFT is:  [insert number and identification of each lot, if applicable]  

	

	ITT 1.2
	The expected Completion Date of the Works is: Eight (8) calendar months from the date of commencement  
	

	ITT 2.1
	Name of financing institution is: DACF (Kintampo Municipal Assembly)
	

	ITT 5.2(c)
	Equipment which shall be required for the execution of the assignment are:
	No.
	Equipment Type and Characteristics
	Minimum Number required for contract 

	1
	Tipper Truck 18 cubic meter 
	1

	2
	Pick Up
	1

	3
	Concrete Mixer
	1

	4
	Plate Compactor
	1

	5
	Tubular Scaffolds 
	10 sets

	6
	Wheelbarrows
	10

	

	
Requisite key personnel with the qualification and experience as follows;

	Position
	Minimum
Qualification
	Min. Years of Experience

	Contract Manager
	BSc / B-Tech / HND 
Civil Engineering / 
Building Technology
	BSc -5Years

HND-8years 

	Project Engineer
	BSc / B-Tech / HND in Civil Engineering / 
Building Technology
	BSc -5Years

HND-7years

	Works 
Superintendent 
	CTC II (OLD
SCHEME) / CTC III
	5Years











	

	[bookmark: _Toc240918341]B.  Request for Quotation Documents
	

	ITT 9.1
	For purposes of clarification, the Employer’s address:
 Municipal Coordinating Director
Kintampo Municipal Assembly 
P. O. Box 20, Kintampo – Bono East Region
Tel: 0244884712
Email: info@kima.gov.gh
The minimum number of days prior to the deadline for submission of Request for Quotations to receive any request for clarification Seven (7) days from date of tender submission 
The minimum number of days prior to the deadline for submission of Request for Quotations that the Employer will respond:  Six (6) days
The responses shall not be posted on the Employer’s website.     
	

	[bookmark: _Toc240918342]C.  Preparation of Request for Quotations
	

	ITT 12.1(g)  
	The Request for Quotation Prospective Contractor shall submit with its Request for Quotation the following additional documents:
a. Evidence of Similar works executed in the last three (3) years
b. Audited Accounts for the last three years
c. Key Personnel
d. Information on Plant and Equipment                                                 
	

	ITT 12.2 (g)
	Average Annual Construction Turnover: Minimum average annual construction turnover for each year as set forth below, calculated as total certified payments received for contracts in progress or completed, within last 3 years. 
(i) For Award of this Contract: GH₡2,830,773.38 or equivalent.

	

	ITT 12.2(g)
	Financial Resources: Tenderer must demonstrate access to, or availability of, financial resources such as liquid assets, unencumbered real assets, lines of credit, and other financial means, other than any contractual advance payments to meet the following cash-flow requirement:   
(i) For Award of this Contract:   
GH₡188,718.23
	

	ITT12.3 (g)
	Submission of audited financial statements, including balance sheets, cash flow statements, or income statements or, if not required by the laws of the Applicant’s country, other financial statements acceptable to the Employer, for the last Three years to demonstrate the current soundness of the Tenderer’s
Financial position and its prospective long-term profitability. N/A
(i)Average coefficient of Current ratio (Current Assets /Current Liabilities): > 1.2 -N/A
(ii) Average coefficient of Debt Ratio (Total Debt/Total Assets) < 0.75 N/A
	

	ITT 13.4

	The prices quoted by the Request for Quotation Prospective Contractor shall not be subject to adjustment during the performance of the Contract. 
	

	ITT 14.1
	The currency(ies) of the Request for Quotation shall be as follows:  Ghana Cedis (GHS)  
The currency (ies) of the payment shall be as follows: [Ghana Cedis (GHS)]

	ITT 15.1
	The Request for Quotation validity period shall be 28 days.

	ITT 16.1
	A Request for Quotation Securing Declaration [insert “shall” or “shall not”] be required.
The form of the Request for Quotation Securing Declaration shall be: [insert requirement here] 

	ITT 16.2
	The amount and currency of the Request for Quotation Security shall be: All Tenders must be accompanied by a Tender Security in the form and amount specified in the Tender Advert or 2% of the Tender Sum. Tenders shall be valid for a period of 120 days after Tender opening.

	ITT 17.2
	The written confirmation of authorization to sign on behalf of the Request for Quotation Prospective Contractor shall consist of:  Power of Attorney
The name and description of the documentation required to demonstrate the authority of the signatory to sign the Request for Quotation such as Power of Attorney

	[bookmark: _Toc240918343]D.  Submission of Request for Quotations

	
	

	ITT 18.2(b)
	For Request for Quotation submission purposes only, the submission address is: Electronically through GHANEPS
ADDRESS OF EMPLOYER:
Street Address:  BK-00013 -2941                    
Building Name:  Kintampo Municipal Assembly                                                      
City/Town:  Kintampo                         
Country:  Ghana
Email: Info@kima.gov.gh   
Attention:                                                                                   
  GHANEPS. https://www.ghaneps.gov.gh/epps/app/searchplan.do
                              

	ITT 19.1 
	The deadline for Request for Quotation submission is:
Day:  Monday
Date:  19th October, 2026
Time: 10:00 hrs. GMT

	[bookmark: _Toc240918344]E.  Request for Quotation Opening and Evaluation

	ITT 22.1
	The Request for Quotation opening shall take place at:
Date: 19th October, 2026 
Time: 10:00hrs GMT (Local Time)
Procedure for electronic opening: Procedure for electronic opening:  Tenders will be opened immediately after the deadline for submission on the GHANEPS. https://www.ghaneps.gov.gh/epps/app/searchplan.do

	ITT 27.1
	The currency that shall be used for Request for Quotation evaluation and comparison is: Ghana Cedis (GHS)

	[bookmark: _Toc240918345]F.  Award of Contract
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The shortlist of the prospective contractors was based on their competence in the following:
Equipment holding;
Adequacy of Capital;
Key Personnel;
Workload, among others.
The evaluation shall therefore be based on Price.
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[bookmark: _Toc240918348]1.  Contractor’s Request for Quotation
[The Prospective Contractor shall fill in and submit this Request for Quotation form with the Request for Quotation.  
[date]
Identification No. and Title of Contract: [insert identification number and title of the Contract]
To: 	The Hon. Municipal Chief Executive
             Kintampo Municipal Assembly
             P. O. Box 20
             Kintampo - Bono East Region      
Having examined the Request for Quotation Documents, including addenda [insert list], we offer to execute the contract for the construction of 1No. CHPS Compound at Alhassan Akra in the Kintampo Municipality in accordance with the form of Contract accompanying this Request for Quotation for the Contract Price of [insert amount in numbers], [insert amount in words] [insert name of currency]. The total amount of all Taxes and Duties, not included within the above Quotation Price, has been assessed to be the sum of [insert amount in figures and words] as per the attached Schedule of Prospective Contractor’s Local Tax and Duty Assessment.
The Contract shall be paid in the following currencies:
	Currency
	Percentage payable in currency
	Rate of exchange:  one [insert foreign] equals [insert local]
	Inputs for which [insert foreign] is required

	(a)

(b)
	
	
	



Our Quotation shall be valid for the period of time in accordance with the RQDS, from the date fixed for Quotation submission deadline in accordance with the RQDS, and it shall remain binding upon us and may be accepted at any time before the expiration of that period.  

We have no conflict of interest.
Our firm, its affiliates or subsidiaries—including any subcontractors or suppliers for any part of the Contract—has not been declared ineligible the World Bank, or under the Employer’s country laws or official regulations or as otherwise provided in RQDS. 

Commissions or gratuities, if any, paid or to be paid by us to agents relating to this Request for Quotation, and to Contract execution if we are awarded the Contract, are listed below:
	Name and address of agent
	
	Amount and Currency
	
	Purpose of Commission or gratuity

	
	
	
	
	

	
	
	
	
	

	(if none, state “none”)



We understand and agree that this Request for Quotation and your written acceptance of it shall constitute a binding Contract between us.  We understand that you are not bound to accept the lowest or any Quotation you receive.

Authorized Signature: ……………………………………………………………………………………………………………
Name and Title of Signatory: ………………………………………………………………………………………………….
Name of Request for Prospective Contractor: ……………………………………………………………………………………………………………….
Address: ……………………………………………………………………………………………………………………………….
Date: .…..……………………………………………………………………………………………………………………………….
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Table B.  Withholding Tax
	Item
	Description
	Rate
	Applicable Value
	Total Tax Due

	1
2
	Foreign Component
Local Component
	
	
	



Table C.  Summary
TOTAL AMOUNT OF ALL TAXES CARRIED TO LETTER OF REQUEST FOR QUOTATION: [insert amounts in numbers and in words in currency]
Import Duties			_____________________
VAT 
GET Fund
NHIL			_____________________
Withholding Tax		_____________________
     Total			_____________________
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[bookmark: _Toc240918350]Section V.  General Conditions of Contract

Agreement
The Employer is ____________________________________________________________ of ___________________________________________________________________________
The Contractor is ____________________________________________________________ of ___________________________________________________________________________
The Employer desires the execution of certain Works known as ________________________
____________________________________________________________________________
OFFER
The Contractor has examined the documents listed in the Appendix which forms part of this Agreement and offers to execute the Works in conformity with the Contract for the sum of _____________________________________________________________________ (in words)
________________________________ (in figures) (_________________________________)
or such other sum as may be ascertained under the Contract.
This offer, of which the Contractor has submitted two signed originals, may be accepted by the Employer by signing and returning one original of this document to the Contractor before ________________________________________________________________________ (date) 
The Contractor understands that the Employer is not bound to accept the lowest or any offer received for the Works.

	Signature: ___________________________

	Date: _______________________________

	Name: ______________________________

	Authorized to sign on behalf of (organization name): ______________________________

	Capacity:____________________________

	____________________________________



ACCEPTANCE
The Employer has by signing below, accepted the Contractor’s offer and agrees that in consideration for the execution of the Works by the Contractor, the Employer shall pay the Contractor in accordance with the Contract. This Agreement comes into effect on the date when the Contractor receives one original of this document signed by the Employer.

	Signature: ___________________________

	Date: _______________________________

	Name: ______________________________

	Authorized to sign on behalf of (organization name): ______________________________

	Capacity:____________________________


	____________________________________






General Conditions
1. General Provisions

	1.1	
Definitions
	In the Contract defined below, the words and expressions defined shall have the following meanings assigned to them, except where the context requires otherwise:


	The Contract
	1.1.1 “Contract” means the Agreement and other documents listed in the Appendix.


	
	1.1.2	 “Specification” means the document as included in the Appendix, including Employer’s Requirements in respect of design to be carried out by the Contractor, if any, and Variation to such document. 

	
	1.1.3	“Drawings” means the Employer’s drawings of the Works as listed in the Appendix, and any Variation to such drawings.


	Persons
	1.1.4	“Employer” means the person named in the Agreement and the legal successors in title to this person, but not (except with the consent of the Contractor) any assignee.


	
	1.1.5	“Contractor” means the persons named in the agreement and the legal successors in title to this person, but not (except with the consent of the Employer) any assignee.


	
	1.1.6	“Party” means either the Employer or the Contractor, as the context requires. 

	Dates, Times
and Periods 

	1.1.7	“Commencement Date” is 7 days after date of site possession or any other date agreed between the parties.


	
	1.1.8	“day” means a calendar day. 


	
	1.1.9 “Time for Completion” means the time for completing the Works as stated in the Appendix (or as extended under Sub-Clause 7.3), calculated from the Commencement Date.


	Money and
 Payments
	1.1.10“Cost” means all expenditure properly incurred (or to be incurred) by the Contractor, whether on or off the Site, including overheads and similar charges, but does not include profit.


	Other Definitions
	1.1.11“Contractor’s Equipment” means all apparatus, machinery, vehicles, facilities and other things required for the execution of the Works but does not include Materials or Plant.


	
	1.1.12	“Country” means the country in which the Site is located.


	
	1.1.13“Employer’s Liabilities” means those matters listed in Sub-Clause 6.1.


	
	1.1.14“Force Majeure” means the an exceptional event or circumstance: which is beyond a Party’s control; which such Party could not reasonably have provided against before entering into Contract; which, having arisen, such Party could not reasonably have avoided or overcome; and, which is not substantially attributable to the other Party.


	
	1.1.15	“Materials” means things of all kinds (other than Plant) intended to form or forming part of the permanent work.


	
	1.1.16 “Plant” means the machinery and apparatus intended to form or forming part of the permanent work.


	
	1.1.17 “Site” means the places provided by the Employer where the Works are to be executed, and any other places specified in the Contract as forming part of the Site.


	
	

	
	1.1.19 “Works” means all the work and design (if any) to be performed by the Contractor including temporary work and any Variation.




1.2	
Interpretation		Words importing persons or parties shall include firms and 
organisations. Words importing singular or one gender shall
include plural or other gender where the context requires.  

1.3	
Priority of Documents	The documents forming the Contract are to be taken as mutually explanatory of one another.  If an ambiguity or discrepancy is found in the documents, the Employer shall issue any necessary instructions to the Contractor, and the priority of the documents shall be in accordance with the order as listed below:

1.4	
Law	The law of the Contract is Law of Ghana
			

1.5	
Communications 	wherever provision is made for the giving or issue of any notice, instruction, or other communication by any person, unless otherwise specified such communication shall be written in the language stated in the English Language and shall not be unreasonably withheld or delayed.

1.6	
Statutory Obligation 	The Contractor shall comply with the laws of Ghana. The Contractor shall give all notices and pay all fees and other charges in respect of the Works.
 

2.	The Employer
 
2.1	Provision of Site	The Employer shall provide the Site and right of access thereto within 14 days from the date of signing the contract.
 
2.2	
Permits and Licenses	The Employer shall, if requested by the Contractor, assist him in 
applying for permits, licenses or approvals which are required for the Works.
			
2.3
Employer’s Instructions	The Contractor shall comply with all instructions given by the Employer in respect of the Works including the suspension of all or part of the Works.

2.4	
Approvals 	No approval or consent or absence of comment by the Employer or the Employer’s representative shall affect the Contractor’s obligations.



3.	The Employer’s Representatives

3.1	Authorised Person 
	One of the Employer’s personnel shall have authority to act for him. This authorized person shall be (insert name and position) 


3.2	
Employer’s Representative	The Employer may also appoint a firm or individual to carry out certain duties. The appointee (name of firm or individual) The Employer shall notify the Contractor of the delegated duties and authority of this Employer’s representative.



4.    The Contractor

4.1 General Obligations	The Contractors shall carry out the Works properly and in 
accordance with the Contract. The Contractor shall provide all supervision, labour, Materials, Plant and Contractor’s Equipment which may be required. All materials and Plant on Site shall be deemed to be the property of the Employer.

4.2	
Contractor’s	The Contractor shall submit to the Employer for consent the name
Representative 	and particulars of the person authorized to receive instructions on behalf of the Contractor.
		
Employer’s Liabilities 	In this Contract, Employer’s Liabilities mean:
				
a) War, hostilities (whether war be declared or not), invasion, act of foreign enemies, within the Country,
b) Rebellion, terrorism, revolution, insurrection, military or usurped power, or civil war, within the Country,
c) Riot, commotion or disorder by persons other than the Contractor’s personnel and other employees, affecting the Site and/or the Works,
d) Ionizing radiations, or contamination by radio-activity from any nuclear fuel, radio-active toxic explosive, or other hazardous properties of any explosive nuclear assembly or nuclear component of such an assembly, except to the extent to which the Contractor may be responsible for the use of any radio-active material,
e) Pressure waves caused by aircraft or other aerial devices travelling at sonic or supersonic speeds,
f) Use or occupation by the Employer of any part of the Works, except as may be specified in the Contract,
g) Design of any part of the Works by the Employer’s personnel or by others for whom the Employer is responsible, and 
h) Any operation of the forces of nature affecting the Site and/or the Works, which was unforeseeable or against which an experienced Contractor could not reasonably have been expected to take precautions,
i) Force Majeure,
j) A suspension under Sub-Clause 2.3 unless it is attributable to the Contractor’s failure,
k) Any failure of the Employer,
l) Physical obstructions or physical conditions other than climatic conditions, encountered on the Site during the performance of the Works, which obstructions or conditions were not reasonably foreseeable by an experienced Contractor and which the Contractor immediately notified to the Employer,
m) Any delay or disruption caused by any Variation,
n) Any change to the law of the Contract after the date of the Contractor’s offer as stated in the Agreement,
o) Losses arising out of the Employer’s right to have the permanent work executed on, over, under, in, or through any land, and to occupy this land for the permanent work, and
p) Damage which is an unavoidable result of the Contractor’s obligations to execute the Works and to remedy any defects.
	



7.	Time for Completion

7.1		
Execution of the Works 	The Contractor shall commence the Works on the Commencement Date and shall proceed expeditiously and without delay and shall complete the Works within the Time for Completion.
	 
7.2		 
Programme  	Within 7 days from the commencement date the Contractor shall submit to the Employer a programme for the Works. 
7.3		
Extension of Time 		Subject to Sub-Clause 10.3, the Contractor shall be entitled to an 
extension to the Time of Completion if he is or will be delayed by any of the Employer’s Liabilities.

On receipt of an application from the Contractor, the Employer shall consider all supporting details provided by the Contractor and shall extend the Time for Completion as appropriate.

7.4		
Late Completion 	If the Contractor fails to complete the Works within the Time for Completion, the Contractor’s only liability to the Employer for such failure shall be to pay 0.02% for each day for which he fails to complete the Works.



8.	Taking-Over

8.1		
Completion 		The Contractor may notify the Employer when he considers that 
the Works are complete.

8.2		
Taking-Over Notice	The Contractor shall notify the Employer when he (the Contractor) Considers that the Contractor has completed the Works stating the date accordingly. Alternatively, the Employer may notify the Contractor that the Works, although not fully complete, are ready for taking over, stating the date accordingly. The Employer shall take over the Works after successful inspection.

	


9.	Remedying Defects 

9.1		
Remedying Defects 	The Employer shall notify the Contractor of any defects or outstanding Works within 28 days after taking over. . The Contractor shall remedy at no cost to the Employer any defects due to the Contractor’s design, Materials, Plant or workmanship not being in accordance with the Contract.

The cost of remedying defects attributable to any other cause shall be valued as a Variation. Failure to remedy any defects or complete outstanding work within a reasonable time of the Employer’s notice shall entitle the Employer to carry out all necessary work at the Contractor’s cost.

9.2		
Uncovering and Testing 	The Employer may give instruction as to the uncovering and/or testing of any work. Unless as a result of any uncovering and/or testing it is established that the Contractor’s design, Materials, Plant or workmanship are not in accordance with the Contract, the Contractor shall be paid for such uncovering and/or testing as a Variation in accordance with Sub-Clause 10.2.


10.	Variations and Claims

10.1		
Right to Vary 		the Employer may instruct Variations.
	

10.2		
Valuation of Variations 	 shall be valued as follows:  								
a)  at a lump sum price agreed between the Parties, or

b) where appropriate, at rates in the Contract, or
 
c) in the absence of appropriate rates, the rates in the Contract shall be used as the basis for valuation, or falling which

d) at appropriate new rates, as may be agreed or which the Employer considers appropriate, or 

e) if the Employer so instructs, at daywork rates set out in the Appendix for which the Contractor shall keep records of hours of labour and Contractor Equipment, and of Materials used. 

10.3		
Early warning 	 	A Party shall notify the other as soon as he is aware of any 
circumstances which may delay or disrupt the Works, or which may give rise to a claim for additional payment. The Contractor shall take all reasonable steps to minimize these effects.
	
The Contractor’s entitlement to extension to the Time of Completion or additional payment shall be limited to the time and payment which would have been due if he had given prompt notice and had taken all reasonable steps.

10.4		
Right to Claim		If the Contractor incurs Cost as a result of any of the Employer’s 
Liabilities, the Contractor shall be entitled to the amount of such Cost. If as a result of any of the Employer’s Liabilities, it is necessary to change the Works, this shall be dealt with as a Variation. 
10.5		
Variation and Claim		The Contractor shall submit to the Employer an itemized make-up 
Procedure 			of the value of Variations and claims within 28 days of the 
instruction or of the event giving rise to the claim. The Employer shall check and if possible, agree the value. In the absence of agreement, the Employer shall determine the value. 
						 	
	

11.	Contracts Price and Payment
 	
11.1		
Valuation of the Works	The Works shall be valued as provided for in the Works Requirements, 
subject to Appendix III.


11.2		
Monthly Statements 	           The Contractor shall be entitled to be paid at monthly intervals: 
	
the value of the Works executed,

subject to any additions or deductions which may be due.

The Contractor shall submit each month to the Employer a statement showing the amounts to which he considers himself entitled.

11.3		
Interim Payments 		Within 28 days of delivery of each statement, the Employer shall 
pay to the Contractor the amount shown in the contractor’s statement less retention at the rate of 5% of the value of the monthly statement and less any amount for which the Employer has specified his reasons for disagreement. The cumulative retention deducted shall not exceed 5% of the total contract price. The Employer shall not be bound by any sum previously considered by him to be due to the Contractor.
	
11.4		

11.5		
Payment of Second Half of  	The full retention shall be paid by the Employer to the 
Retention 			Contractor within 14 days after 
the remedying of notified defects or the completion of outstanding work, all as referred to in Sub-Clause 9.1, whichever is the later.  
		
11.6	
Final Payment 	Within 42 days of the latest of the events listed in Sub-Clause 11.5 above, the Contractor shall submit a final account to the Employer together with any documentation reasonably required to enable the Employer to ascertain the final contract value.

Within 28 days after the submission of this final account, the Employer shall pay to the Contractor any amount due. If the Employer disagrees with any part of the Contractor’s final account, he shall specify his reasons for disagreement when making payment.

11.7
Currency	Payment shall be in Ghana cedi.

11.8		
Delayed Payment 	The Contractor shall be entitled to compound interest at the selling rate for Construction by the Bank of Ghana. The date of exchange rate shall be 28 days prior to the date of due payment. 


12.2		
Default by Employer 	
12.3		
Insolvency  	
12.4		
Payment upon 	After termination, the Contractor shall be entitled to payment of 
Termination 	the unpaid balance of the value of the Works executed and of the Materials and Plants reasonably delivered to the Site, adjusted by the following:
	
a) any sums to which the Contractor is entitled under Sub-Clause 10.4,

b) any sums to which the Employer is entitled,

c) if the Employer has terminated under Sub-Clause 12.1 or 12.3, the Employer shall be entitled to a sum equivalent to 20% of the value of those parts of the Works not executed at the date of the termination, 

d) if the Contractor has terminated under Sub-Clause 12.2 or 12.3, the Contractor shall be entitled to the Cost of his suspension and demobilization together with a sum equivalent to 10% of the value of those parts of the Works not executed at the date of termination.

The net balance due shall be paid or repaid within 28 days of the notice of termination.



13.	Risk and Responsibility
 
13.1		
Contractor’s Care of the 	The Contractor shall take full responsibility for the care of the 
Works 	Works from the Commencement Date until the date of the Employer’s notice under Sub-Clause 8.2. responsibility shall then pass to the Employer. If any loss or damage happens to the Works during the above period, the Contractor shall rectify such loss or damage so that the Works conform with the Contract.
			
Unless the loss or damage happens as a result of an Employer’s Liability, the Contractor shall indemnify the Employer, the Employer’s contractors, agents and employees against all loss or damage happening to the Works and against all claims or expense arising out of or caused by a breach of the Contract, by negligence or by other default of the Contractor, his agents or employees.

13.2		
Force Majeure	If a Party is or will be prevented from performing any of its obligations by Force Majeure, the Party affected shall notify the other Party immediately. If necessary, the Contractor shall suspend the execution of the Works and, to the extent agreed with the Employer, demobilize the Contractor’s Equipment.

If the event continues for a period of 84 days, either Party may then give notice of termination which shall take effect 28 days after the giving of the notice.

After termination, the Contractor shall be entitled payment of the unpaid balance of the value of the Works executed and of the Materials and Plant reasonably delivered to the Site, adjusted as follows:

a) any sums to which the Contractor is entitled under Sub-Clause 10.4,
b) the Cost of his suspension and demobilisation,
c) any sums to which the Employer is entitled.

				The net balance due shall be paid or repaid within 28 days of the 
notice of termination.


14.	Insurance 

14.1		
Extent of Cover		The Contractor shall, prior to commencing the Works, effect and 
thereafter maintain insurances in the joint names of the Parties:

a) for loss and damage to the Works, Materials, Plant and the Contractor’s Equipment,

b) for liability of both Parties for loss, damage, death or injury to third parties or their property arising out of the Contractor’s performance of the Contract, including the Contractor’s liability for damage to the Employer’s property other than the Works, and

c) for liability of both Parties and of any Employer’s representative for death or injury to the Contractor’s personnel except to the extent that liability arises from the negligence of the Employer, any Employer’s representative or their employees. 

14.2		
Arrangements	All insurances shall conform with any requirements detailed in the Appendix. The policies shall be issued by insurers and in terms approved by the Employer. The Contractor shall provide the Employer with evidence that any required policy is in force and that the premiums have been paid.

All payments received from insurers relating to loss or damage to the Works shall be held jointly by the Parties and used for the repair of the loss or damage or as compensation for loss or damage.

14.3		
Failure to Insure	 If the Contractor fails to effect or keep in force any of the insurances referred to in the previous Sub-Clauses, or fails to provide satisfactory evidence, policies or receipts, the Employer may, without prejudice to any other right or remedy, effect insurance for the cover relevant to such default and pay the premiums due and recover the same as a deduction from any other monies due to the Contractor.
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Special Conditions of Contract
The following Special Conditions of Contract (SCC) shall supplement and / or amend the General Conditions of Contract (GCC).  Whenever there is a conflict, the provisions herein shall prevail over those in the GCC.  
	[bookmark: _Toc240918353]A. General

	GCC 1.1.4
	The Employer is: [Insert complete name] 

	GCC 1.1.7
	The Commencement Date shall be: [insert date]

	GCC 1.1.9
	The Intended Completion Date for the whole of the Works shall be [Insert number of days deemed appropriate here] 

	GCC 1.1.17
	The Site is located at [Insert address of Site] and is defined in drawings No.  [Insert numbers]

	
	

	GCC 1.1.19
	The Works consist of: Construction of CHPS Compound at Alhassan Akura


	GCC 1.3
	The following documents constitute the Contract:  [Insert detailed list documents forming the Contract]

	GCC 1.4
	The governing law is that of: The Republic of Ghana

	GCC 1.5
	This Contract shall be executed in the ENGLISH language.     

	GCC 2.1
	The Site Possession Date(s) shall be: [insert location(s) and date(s), as relevant and applicable]

	GCC 3.1 
	The Employer’s authorized person for the purpose of communications shall be:  [state full name, address, telephone, fax and e-mail] 

	GCC 3.2
	The Employer’s Representative shall be: [state full name, address, telephone, fax and e-mail]

	GCC 4.2
	The Contractor’s authorized person for the purpose of communications shall be:  [state full name, address, telephone, fax and e-mail]

	GCC 4.4
	The Performance Security shall be: [insert amount(s) denominated in the types and proportions of the currencies in which the Contract Price is payable, or in a freely convertible currency acceptable to the Employer] in the form of:
Bank Guarantee: [insert percentage and amount(s)]; or 
Performance Bond: [insert percentage and amount(s)].

[A Bank Guarantee shall be unconditional (on demand) (See Section VII–Forms of Agreement and Security).  An amount of 5 to 10 percent of the Contract Price is commonly specified for Performance Bank Guarantees.
 A Performance Bond is an undertaking by a bonding or insurance company (surety) to complete the construction in the event of default by the Contractor, or to pay the amount of the Bond to the Employer.  An amount of 30 percent of the Contract Price is commonly used internationally for this type of security (See Section VII–Forms of Agreement and Security)]

	GCC 5.1 
	 The Contractor shall carry out designs for [insert part of works to be carried out by Contractor]

	GCC 2.1
	The Site Possession Date(s) shall be: [insert location(s) and date(s), as relevant and applicable]

	GCC 2.2
	Permits, approvals and / or licenses, or public service undertakings to be acquired by the Contractor: [Insert full details]

	GCC 3.1
	The authorized person to act on behalf of the Employer shall be: [insert Full name and address].

	GCC 3.2
	The Employer appoints [insert name and address of firm or individual]

	GCC 15.3
	The institution whose arbitration procedures shall be used is: [Stipulate institution whose Rules of Arbitration shall apply]

	[bookmark: _Toc240918354]B. Time Control

	GCC 7.3
	The Contractor shall submit for approval a Programme for the Works within  [Insert number] days from the date of the Letter of Acceptance.

	GCC 7.4
	The Contractor shall pay [insert amount] to the Employer upon failure to complete the Works within the Time for Completion.

	[bookmark: _Toc240918355]C. Quality Control

	GCC 9.1
	The Defects Liability Period is:  [Insert number] days.
[The Defects Liability Period is usually limited to 12 months, but could be less in very simple cases]

	[bookmark: _Toc240918356]D. Cost Control

	GCC 11.3
	The proportion of payments retained is: [Insert percentage]  
[The retention amount is usually to be kept close to 5 percent and shall in no case exceed 10 percent]  

	GCC 11.7
	The currency of the Employer’s country is Ghana Cedis (GHS)  






	GCC 11.8
	The Contractor shall be entitled to interest at [insert percentage] for each day the Employer fails to pay beyond prescribed payment period.

	[bookmark: _Toc240918357]E. Finishing the Contract

	GCC 8.2
	The Employer shall take over the site and the Works immediately after the authorized person issues a Certificate of Completion.





Section VI.  Special Conditions of Contract and Additional Provisions of Contract
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[bookmark: _Toc240918358]Section VII. Forms of Agreement 





[bookmark: _Toc240918359]Section VII. Forms of Agreement 


[This Section contains Contract Forms which, once completed, will constitute part of the Contract. 

Forms include:
· Letter of Acceptance
· Contract Agreement

Letter of Acceptance
[The Letter of Acceptance shall be the basis for formation of the Contract as described in the RQDS.  This Standard Form of Letter of Acceptance shall be filled in and sent to the successful Contractor only after evaluation of Request for Quotations has been completed.]

[Letterhead of the Employer]
 [insert date]

Identification No and Title of Contract: [insert identification number and title of the Contract]
To:  [insert name and address of the Contractor]
This is to notify you that your Quotation dated [insert date] for execution of the [insert name of the Contract and identification number, as given in the Request for Quotation Documents] for the Contract Price of the equivalent[footnoteRef:1] of [insert amount in numbers and words] [insert name of currency], as corrected and modified[footnoteRef:2] in accordance with the Instructions to Prospective Contractors is hereby accepted by the Employer. [1: 	 	Delete “of the equivalent” if the Contract Price is expressed wholly in one currency.]  [2: 	 	Delete “corrected and” or “and modified” if not applicable.  ] 

You are hereby instructed to (a) proceed with the execution of the said Works in accordance with the Contract (b) sign and return the attached Agreement, within 7 days after receipt of this Letter of Acceptance. 
Authorized Signature: 

Name and Title of Signatory:  
[insert proper name of the Employer]
Attachment:  Agreement

[bookmark: _Toc240918360]Contract Agreement

THIS CONTRACT AGREEMENT is made on the 	 day of 	 20 	

BETWEEN

[insert complete name of Employer], a [insert description of type of legal entity, for example, an agency of the Ministry of ...] of the Government of {insert name of Country of Employer}, or corporation incorporated under the laws of {insert name of Country of the Employer} and having its principal place of business at [insert address of Employer] (hereinafter called “the Employer”) of the one part 

And

[Insert complete name of Contractor], a corporation incorporated under the laws of [insert name of Country of the Contractor] and having its principal place of business at [insert address of Contractor] (hereinafter called “the Contractor”) of the other part.

WHEREAS, the Employer Requested for Quotations for the Works, described as Construction of 1No. CHPS Compound at Alhassan Akura in the Kintampo Municipality and has accepted a Quotation by the Contractor for the execution and completion of these Works and the remedying of any defects therein, and the Employer agrees to pay the Contractor the Contract Price or such other sum as may be payable under the provisions of the Contract at the times and in the manner prescribed in the Contract.  

NOW THIS AGREEMENT WITNESSETH as follows:

1.	In this Agreement, words and expressions shall have the same meanings as are respectively assigned to them in the Contract documents referred to.

2.	The documents identified in Sub-Clause 1.3 of the General Conditions of Contract and the Special Conditions of Contract shall be deemed to form and be read and construed together as part of the Contract and the priority of such documents shall be as provided in such Sub-Clause 1.3.

3.	In consideration of the payments to be made by the Employer to the Contractor as provided in the Contract, the Contractor hereby covenants with the Employer to execute and complete the Works and remedy any defects therein in conformity in all respects with the provisions of the Contract.

4.	The Employer hereby covenants to pay the Contractor in consideration of the execution and completion of the Works and the remedying of defects therein; the Contract Price or such other sum as may become payable under the provisions of the Contract at the times and in the manner prescribed by the Contract.


IN WITNESS whereof, the parties hereto have caused this Agreement to be executed the day and year first before written.

The Common Seal of 	 was hereunto affixed in the presence of:
	 or 	

Signed, sealed, and delivered by the said 	
In the presence of:  	



Binding Signature of Employer 	



Binding Signature of Contractor 	









Note: All italicized text (including footnotes) is for use in preparing forms in these Request for Quotation documents and shall be deleted from the final product
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Section VIII: Bills of Quantities                                                   
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[bookmark: _Toc240918363]Bills of Quantities
The Bills of Quantities for this Request for Quotation shall be inserted in this Appendix.























Section VIII. Bills of Quantities		
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[bookmark: _Toc240918364]SPECIFICATIONS AND PERFORMANCE REQUIREMENTS




































[bookmark: _Toc240918365]Specifications
The Specifications for this Request for Quotation shall be inserted in this Appendix.




















Section IX. Specifications and Performance Requirements	
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Section X. Drawings	                                                                
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ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

CONSTRUCTION OF 1NO. COMMUNITY-BASE

HEALTH PLANNING SERVICE (CHPS) COMPOUND

AT ALHASSAN AKURA

BILL No. 2: MAIN WORKS FOR CHPS COMPOUND

SUBSTRUCTURE (ALL PROVISIONAL)

D. GROUNDWORK

D 20: Excavating and Filling

Site Preparation

Clear site of all bush and undergrowth and dispose from site

Cut off trees and uproot stump of girth 600mm-1200mm

Excavating
Topsoil for preservation average depth 150mm deep.

Pit; maximum depth not exceeding 2.0m commencing
from stripping level.

Excavate trench, width exceeding 0.30m for strip
foundation not exceeding 1.0m deep commencing from
stripping level.

Disposal

Disposal off excess excavated material from site including
rock or artificial hard material.

Filling

Backfill using selected excavated material around
foundation in well compacted layers of average thickness
not exceeding 250mm thick arising from foundations.
Hardcore Filling

Provide, place, well levelled and compacted in 150mm
thick layers approved imported fill material to make up
levels to the required density as directed to receive
concrete bed.

E: IN-SITU CONCRETE /LARGE PRECAST CONCRETE

E10: In-situ concrete

Plain ordinary prescribed concrete mix: grade C20 concrete,
20mm aggregate as described in:

Blinding bed, thickness not exceeding 50mm poured
on or against earth

Strip foundation

SUBSTRUCTURE
To Collection

912

650

39

21

22

57

10

SM

Nr

SM

CM

CM

CM

CM

CM

SM

CM

1B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)
SUBSTRUCTURE CONT'D
A ||Bed (concrete), thickness 150mm poured on unblinded 112 || SM
hardcore with fair floated surface
B [[Steps and Ramps 2 CM
Reinforced ordinary prescribed concrete mix: grade C20
concrete, 20mm aggregate filled into formwork and around
reinforcement (both measured separately) as described in:
C [|Column bases 3 CM
D ||Columns 1 CM
E20: Formwork for In-situ concrete
Sawn Formwork to:
E ||Vertical Sides columns 15 SM
F |[Edges of concrete bed, height not exceeding 150mm 43 LM
G ||Vertical sides of steps and risesr 150mm high 15 LM
E30: Reinforcement for In-situ concrete
Mild steel bars reinforcement to BS4449 as describe in:
H  ||12mm Diameter bars in column basese 133 KG
J 12mm Diameter bars in column 74 KG
K ||8Bmm Diameter bars as stirrups in columns 45 KG
F. MASONRY
F10: Brick/Block Walling
Solid sandcrete block work bedded and jointed in
cement and sand (1:4) mortar in:
L ||Foundation wall, 150mm thick, vertical,built against other work 121 SM

To Collection

COLLECTIONS

Page 1B2

Page 2B2

ELEMENT No. 1: SUBSTRUCTURE
TOTAL TO SUMMARY

2B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)

SUPERSTRUCTURE

ELEMENT No. 2: REINFORCED CONCRETE FRAME

E: IN-SITU CONCRETE /LARGE PRECAST CONCRETE

E10: In-situ concrete

Reinforced ordinary prescribed concrete mix: grade C20

concrete, 20mm aggregate filled into formwork and around

reinforcement (both measured separately) as described in:
A |[Beam/Lintel 4 CM
B ||Columns 2 CM
C |[Copng 1 CM

E20: Formwork for In-situ concrete

Sawn Formwork to:
D [[Side and soffit of regular shaped beams/lintel and coping 75 SM
E |[Vertical Sides of rectangular shaped attached to walls 36 SM
F ||Ditto Isolated columns 10 SM

E30: Reinforcement for In-situ concrete

Mild steel bars reinforcement to BS4449 as describe in:
G ||12mm Diameter bars in beams/lintel 358 KG
H  [[12mm Diameter bars in column 210 KG
J  ||22mm Diameter bars in Coping 95 KG
K [[Bmm Diameter bars as stirrups in columns, beams and coping 301 KG

ELEMENT No.2: REINFORCED CONCRETE FRAME
TOTAL TO SUMMARY

3B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH®)

ELEMENT No. 3: WALLS

F. MASONRY
F10: Brick/Block Walling

Solid sandcrete block work bedded and jointed in

cement and sand (1:4) mortar in:

Wall, 150mm thick, vertical,built against other work

ELEMENT No.3: MASONRY
TOTAL TO SUMMARY

ELEMENT No. 4: STRUCTURAL/CARCASSING METAL/

TIMBER
G: STRUCTURAL/CARCASSING METAL/TIMBER

G20: Carpentry/Timber Framing/First Fixing

Supply and fix the ff:

Approved sawn hardwood treated

with approved preservatives

50 x 150mm Ridge piece

50 x 150mm Rafters

50 x 150mm Wall plate

50 x 100mm Purlins

50 x 100mm Hangers or wall plate
50 X 50mm Ceiling joist/Noggings

\Wrought Hardwood

25 x 250mm Fascia and verge board with chamfered edge
nailed to hardwood

ELEMENT No. 4: STRUCTURAL/CARCASSING METAL/TIMBE

TOTAL TO SUMMARY

321

28

121

78

220

119

401

83

SM

LM

LM

LM

LM

LM

LM

LM

4B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

ELEMENT No. 5: CLADDING/COVERING

H. CLADDING/COVERING

H60: Plain roof sheet

Corrugated aluminium sheet roofing

0.40mm gauge IBR long span corrugated Aluzinc roofing sheet laid with

150m

corrrugations side laps and 150mm end laps on hardwood

purlins , (recommended Manufacturer)

Roof coverings, pitch not exceeding 45°

Extra-over roof covering for Ridge cap

ELEMENT No. 5: CLADDING/COVERING
TOTAL TO SUMMARY

ELEMENT No.6 LINNING/SHEATING/DRY PARTITIONING

202

26

K31: Plasterboard fixed partitions/Liner walls/linning

Approved ordinary polished plywood cut to 1200 x 1200mm bays

fixed to hardwood noggings (measured Separately) plain sheet

finishing

to hardwood noggings

Ditto at eaves

6mm thick interior quality V-joined plywood ceiling boarding nailed

CARRIED TO SUMMARY

ELEMENT No.6 LINNING/SHEATING/DRY PARTITIONING

196

28

SM

LM

SM

SM

5B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

ELEMENT No.7WINDOWS/DOORS/STAIRS

L: WINDOWS/DOORS/STAIRS

L10: Windows/Rooflight/Screens/Louvres
Timber Windows

\Wrought hardwood

\Wrought hardwooas deiscrbed

44 x 144mm hardwood window frame plugged to block work or
concrete

38 x 38 stop fillet

20 X 50mm batterns

Screen, Borrow Lights and frames

Fibre mesh mosquito-proof screen, vertical cut to size and fixed
with batterns (measured separately) to hardwood

Louvre and Frames

An approved Louvre carriers with screws to match

Louvre carrier 1143mm long with clips for 8No. Blade with dual
control

Louvre carrier 513mm long with clips for 4No. Blade with single
control

Burglar-Proofing

14mm mild steel bars cut to specifiied length and threaded
througth holes in hardwood frame at 150mm centers as burglar-
proofing including anti-rust and gloss oil painting

50 X 50mm square steel mesh cut to size fixed to window frame
with batterns (measured separately)

L20:Door/Sheeting/Hatches

metal doors

china or turkey's door

1500 x 2050mm (finished) one and half leaf door

800 x 5050mm (finished) single leaf door

700 x 2050mm (finished) single leaf door

To Collection

76

43

143

21

24

110

32

11

LM

LM

LM

SM

pairs

NR

LM

SM

NR

NR

NR

6B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

ELEMENT No.7 WINDOWS/STAIRS CONT'D

L21:Metal Door/Sheeting/Hatches

1200 x 1550mm galvanized steel gate (double leaf)

L40: General Glazing

Louvres

6mm thick rounded edge louvre obscured 150mm wide including

cutting blades to exact length and grind polishing exposed

Louvre blade 900mm long

To Collection

COLLECTIONS

Page 6B2

Page 7B2

ELEMENT No.7WINDOWS/DOORS/STAIRS
CARRIED TO SUMMARY

207

NR

NR

7B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)

ELEMENT No.8: SURFACE FINISHES

M:SURFACE FINISHES

M10: Sand:cement/Concrete screeds/Toppings

Cement-Sand (1:4); screeded beds/backings
A ||25mm thick screeded beds on top of concrete floor bed

(measured separately) to receive floor tiles 165 || SM
B ||12mm thick screeded backing to receive wall tiles 54 SM
C |[25mm thick screeded backing to receive floor tiles on 300mm treg| 3 SM
D [|Ditto on 150mm risers 2 SM
E ||Ditto on ramps 4 SM

M20: Plastered/Rendered/Roughcast coatings

\Wall Finishings

Plastering/ Rendering

Cement and sand (1:4) mortar render as described:
F  [[19mm thick on Block wall or concrete wall 432 SM
G |[[Ditto Isolated column 9 SM

M40: Stone/Concrete/Quary/Ceramic Tliling/Mosaic

400 x 400mm polished Ceramic floor tiles of approved colour

bedded and jointed in adhesive on cement and sand mortar (1:4)

screeded bed (Measured Separately) level and falls not exceeding

15° from horizontal
H [|8mm thick ceramic Floor tiles 165 SM
J  ||Ditto 125mm high as Floor skirting 65 LM

300 x 300mm unpolished Ceramic floor tiles of approved colour

bedded and jointed in adhesive on cement and sand mortar (1:4)

screeded bed (Measured Separately) level and falls not exceeding

15° from horizontal
K |[Bmm thick ceramic Floor tiles 10 SM
L ||Ditto on tread 3 SM
M |[Ditto on risers 2 SM
N [[Ditto on ramps 4 SM

To Collection

8B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

ELEMENT No.8: SURFACE FINISHES CONT'D
Decorative Strips

Approved decorative strips cut and fixed to concrete edge of riser
200 X 300mm Ceramic wall tiles of approved colour bedded and
jointed in adhessive on cement and sand mortar (1:4) screeded
bed (Measured Separately) level and vertical in:

8mm thick Tiling to walls

M60: Painting/Clear finishing

Prepare and apply one thinned undercoat and two full finishing

coats of ordinary emulsion paint on general surfaces

Rendered/Plastering walls (internally/externally)

Soffit of Ceiling plywood

Prepare and apply one undercoat and two finishing coats

of gloss oil paint on:

General Surfaces of woodwork girth > 300mm

Surfaeces of block/ concrete work

Primer

Prepare and apply two coats of aluminuim wood primer on
back of hardwood joinery before fixing; not exceeding
300mm girth

Prepare and apply one undercoat of anti-rust paint and

two finishing coats of oil on:

Metal surfaces

To Collection

COLLECTIONS

Page 8B2

Page 9B2

ELEMENT No. 8: SURFACE FINISHES
TOTAL TO SUMMARY

44

432

115

54

33

46

54

LM

SM

SM

SM

SM

SM

LM

SM

9B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

>

ELEMENT No. 10: FURNITURE EQUIPMENT
N10: GENERAL FIXTUR/EQUIPMENTES/FURNISHING

Suplly and fix 300 x 750mm mirrior in bathroom

Including a provisional sum of (GHc 70,000.00) for the supply
of the f.f: Office Table 3 No. (1,200mmx900mm) with side
drawers and laidwith leather on top, 1 No 4 in 1 steel benches, 1
No. Medical Examination Bed, 1 No. Delivery Bed, 2 No,
Patient Bed, 2 No. Bedside Storage Cabinet, 1 Set Delivery
Kit, 1 No. Bedscreen, 2 No. BP apparatus, 2 No. Stethescope,
1 No. Digital Thermometre, 2 No. Weighing Scale (kids and
adult), 1 No. Wheel Chair, 2 No. Padal Waste Bin, 1 No.
Double bed, 1 No. Double matresses

ELEMENT No. 10: FURNITURE EQUIPMENT

CARRIED TO SUMMARY

NR

70,000.00

70,000.00

10B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

ELEMENT No. 11: PLUMBING AND ENGINEERING
INSTALLATION

Overflow pipe: PVC pipes and fittings in chase and soil

Include Provisional Sum of GH¢ 5,000.00 for all pipe works
including PVC bends, Tees copper pipes and all ancillaries
associated with installation of all sanitary appliances

SANITARY APPLIANCES

Supply and fix the following sanitary appliances including

assembly and jointing

Low level Water Closet suit comprising vitreous China wash pan
with 'P' OR 'S' trapped plugged and over two gallons vitreous
China Cistern and fixing on pair of consealed wall steel brackets
plugged and screw to blockwork and flush pipe jointing to cistern
and pan

450 x 450mm white vitreous China hand wash basin with 1No.
Chromiun plated pillar taps and waste fittings stray chain and
plug, soap recess and gap overflow and fixing on pair of mild
steel cantilever brackets plugged and screwed to block/concrete
work

Chromium plated toilet roll holder plugged and screwed to
block/concrete wall

20mm diameter chromium plasted Towel Rail 675mm long with

pair of loose brackets screewed to blockwork

Floor drain with both telephone and wall shower rose complete,
taps traps etc, concealed in floor bed

ELEMENT No. 11: PLUMBING AND ENGINEERING
INSTALLATION

CARRIED TO SUMMARY

NR

NR

NR

NR

NR

5,000.00

11B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)
ELEMENT NO. 12: ELECTRICAL INSTALLATIONS
V: ELECTRICAL SUPPLY/POWER LIGHTING SYSTEMS
Switch Gear
Supply and Install The following
A ||6-Way TPN Main Distribution Board complete with 200A
integral switch as Memshield with 4No. 63A miniature breaker 1 NR
B ||30A Cut-Out with fuse 1 NR
C ||warm pin and D-iron 4 NR
Feeder Cable
D {[10Omm PVC Insullated copper cable (Approximate lengh) 75 LM
Wiring of Points
Supply and wire in concealed conduit lighting, Fan, and
Socket outlet points using PVC insullated copper cable as
'Kabel Metal' make or approved equal
E ||Lighting and fan points using 1.5mm? PVC cable 17 NR
F |[13A Socket outlet points using 2.5mm? PVC cable complement
2.5mm?2 yellow/green as earth 10 NR
Luminaries and Accessories
G ||[Energy saving bulb with its accessories 17 NR
H  |[British type ceiling rose 7 NR
J  ||lLamp Holder 17 NR
Power Installation
Switches
Lighting switches 6A single pole silent action flush ivory plastic
plate, steel knock out box plugged and screwed to blockwall
K ||l2-Way 2-Gang Switch 2 NR
L [[1-Way 2-Gang Switch 6 NR
M  [[1-Way 3-Gang Switch 1 NR
N ||1-Way 1-Gang Switch 2 NR

To Collection

12B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)

ELEMENT NO. 12: ELECTRICAL INSTALLATIONS CONT'D
Socket Outlets

A ]2 x 13A Socket outlet 10 NR
Ventilation/Aircondtion System
Supply and fix ceiling fan complete with requlator and hook as
specified

B Ceiling Fan 7 NR
Earthing Protection

C Supply and install complete Earthing protection systerm for the
building as specified 1 NR

D [[Allow for Builders work in connection with the electrical
installation item |[ Sum

To Collection

COLLECTIONS

Page 12B2

Page 13B2

ELEMENT NO. 7: ELECTRICAL INSTALLATIONS
TOTAL TO SUMMARY

13B2








ITEM

DESCRIPTION

QTY

UNIT

RATE
(GH¢)

AMOUNT
(GH¢)

EXTERNAL WORKS

CONSTRUCTION OF APRON

Excavations

Excavate foundation trench not exceeding 300mm deep ¢
commencing at formation level

Backfill selected excavated material around foundation

Remove supluse excavated material

Hardcore filling

Approved imported laterite of hardcore filling as described
To make up levels under bed, deposited, spread and compacted in
layers not exceeding 225mm thick

CONCRETE WORKS

Plain in-situ concrete (1:3:6-20mm aggregate) in:

Foundation trenches

75mm thick concrete apron bed

Formwork to:

Edges of bed, 75mm high

BLOCK WORK

Solide sandcrete blockwall in cement and sand (1:4) mortar in:

125mm thick wall

In-situ Finishing
20mm thick cement and sand (1:4) rendering to blockwork of

concretework on

External wall

Cement and Sand screeded bed (1:3) mortar

50mm thick screeded bed laid to slop on apron

To Collection

19

48

29

19

26

CM

CM

CM

CM

SM

LM

SM

SM

SM

14B2








ITEM DESCRIPTION QTY ||UNIT RATE AMOUNT
(GH¢) (GH¢)
APRON CONT'D
Painting and Decorating
Prepare and apply three coats of approved gloss oil paint on:
A |IRendered walls 26 SM 28.00

To Collection

COLLECTIONS

Page 15B2

Page 16B2

CONSTRUCTION OF APRON

CARRIED TO SUMMARY

15B2








ITEM DESCRIPTION QTY [[UNIT RATE AMOUNT
(GH¢) (GH¢)
A BILL NO. 1 PRELIMINARIES
BILL NO. 2 MAIN WORKS
A |[ELEMENT No. 1 SUBSTRUCTURE (ALL PROVISIONAL)
B ||ELEMENT No. 2 REINFORCED CONCRETE FRAME
C |[[ELEMENT No. 3 MASONARY
D |[[ELEMENT No. 4 STRUCTURAL/CARCASSING/METAL/TIMBER
E |[ELEMENT No. 5 CLADDING/COVERING
F  |[ELEMENT No. 6 LINNING/SHEATHING/DRY PARTITIONING
G |[ELEMENT No. 7 WINDOWS/STAIRS
H ||ELEMENT No. 8 SURFACE FINISHES
J ELEMENT No. 9 FURNITURE AND EQUIPMENT
K [ELEMENT No. 10 PLUMBING AND ENGINEERING WORKS
L |[ELEMENT No. 11 ELECTRICAL INSTALLATIONS
M ||CONSTRUCTION OF APRON

TO FORM TENDER

16B2












COMPLETE CHPS COM. BOQ-WKS AND PRELI.-ALHASSAN AKURA/PRELIMINARIES.pdf

ITEM DESCRIPTION AMOUNT GHC
BILL No. 1
(PRELIMINARIES)

Setting out

A Setting out for the work in accordance with the work drawings
Photo

B Progress photo
Site meeting

C Site progress meeting will be held when required by the consultants and shall be
attended by all the parties to the contractor or their representatives.
Water for works

D Include for provision the amount of water required for the execution of the works
including paying all fees and charges in connection, providing all temporary
distributions, make good of all work disturbed
Temporary stores

E Hire or construct temporary place as a store
Transport for the work

F Allow for the cost in connection with the provision of transport for people at work
First Aid equipment

G The contractor shall provide adequate First Aid equipment which shall be available for
the use of workmen during hours.
Watching and lighting

H The contractor at the time of being placed in possession of the site must include for
watching, lighting and protecting the works, the site and surrounding property by day
and by night including Sundays and holidays
Signboard

J The contractor is to allow for providing a timber notice board size 1.22m x 991mm
overall in a prominent position on the site bearing the title of the project, the names of
the Employer and Consultant in such order and other information as the consultant
may direct
Cleaning the works

K Allow cleaning down the whole premises including glass both sides and cleaning for
floors, paving, metal work finishing and fixtures throughout, cleaning all sanitary
fitting removing all stains dirt and surplus material and rubbish and leaving the works
and site in clean and tidy condition and ready for immediate use, with all damage to
property roads, path and drains etc made good to the satisfactory of the consultant
Progress schedule and working program

L The contractor shall submit a working program for the consultant’s approval

immediately after signing the contract and shall keep this chart as the works proceed
and shall supply to the consultant four copies of a monthly progress report to the
satisfaction of the consultant

TOTAL TO GENERAL SUMMARY
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